SECTION 08 33 13

COILING COUNTER DOORS

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2013 - 2021 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* Wayne Dalton; Coiling counter door products.

This section is based on the products of Wayne Dalton, which is located at:
2501 S. State Highway 121 Bus.
Suite 200
Lewisville, TX 75067
Toll Free Tel: 800-827-3667;
Web Site: www.wayne-dalton.com
Email: info@wayne-dalton.com
[[click here](http://www.arcat.com/arcatcos/cosXX/arcXXXXX.html)] for additional information.
Since its inception in 1954, Wayne-Dalton has become known as a company with innovative ideas, which far exceed industry standards. Often, Wayne-Dalton is the only source for the latest garage door and garage door opener features. Because the company has always maintained a staunch commitment to developing innovative new products, Wayne-Dalton is now a world leader in the garage door and garage door opener industry.
Wayne-Dalton Rolling Doors have a long history of excellence in the design and construction of doors that have met and often exceeded the needs and expectations of even the most critical projects.
With numerous innovations created and experience acquired over the years, Wayne-Dalton continues to lead all other manufacturers with both standard and custom-made doors from a variety of materials and colors to meet almost any need.
So whether it's enormous Titan rolling doors, protective FireStar rolling steel fire doors, ventilated Secur-Vent doors, or secure Accordion-Folding Grilles, you can feel confident that with Wayne-Dalton's many years of knowledge and experience, you will get the best possible solution for your building application needs.
This specification includes 500 Series Shutters for use in applications that incorporate counter tops or openings that require the shutter to rest on a sill. With several different modes of operation including lift-up, awning crank and motor, the Wayne- Dalton Rolling Counter Shutter is the preferred solution for your application. Whether it's a concession stand, accounts payable window, sports arena or school food service, the 500 Series is the counter shutter of choice.

See our SpecWizard:[Click Here](http://www.arcat.com/specwizard/08332way/index.htm)

1. GENERAL
	1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Coiling Metal Counter Doors.
		2. Coiling Metal Counter Doors With Integral Frame
		3. Coiling Counter Fire Doors.
		4. Coiling Counter Fire Doors With Integral Frame.
		5. Coiling Wood Counter Doors.
	1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 05 50 00 - Metal Fabrications.
		2. Section 06 20 00 - Finish Carpentry.
		3. Section 08 71 53 - Security Door Hardware.
		4. Section 09 90 00 - Painting and Coating.
		5. Section 27 05 39 - Surface Raceways for Communications Systems.
		6. Section 26 05 00 - Common Work Results for Electrical.
	1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ASTM A 123 - Standard specification for Zinc (hot-dipped galvanized) coating on iron and steel products.
		2. ASTM A 229 - Standard specification for Steel wire, oil-tempered for mechanical springs.
		3. ASTM A 653 - Standard specification for Steel sheet, zinc-coated (galvanized) by the hot-dipped process, commercial quality.
		4. ASTM A 666 - Standard Specification for Austenitic Stainless Steel Sheet, Strip, Plate, and Flat Bar.
		5. ASTM A 924 - Standard Specification for General Requirements for Steel Sheet, Metallic-Coated by the Hot-Dip Process.
		6. ASTM B 221 - Standard Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Profiles, and Tubes.
		7. NEMA 250 - Enclosures for Electrical Equipment (1000 Volts Maximum).
		8. NEMA MG 1 - Motors and Generators.
		9. NFPA-80 - Standard for Fire Doors and Fire Windows.
	1. DESIGN / PERFORMANCE REQUIREMENTS
		1. Fire Rated Assemblies: Provide assemblies complying with NFPA 80 and listed in UL Directory or Intertek Testing Services (Warnock Hersey Listed) Directory.
	2. SUBMITTALS
		1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
		2. Product Data: Manufacturer's data sheets on each product to be used, including:
			1. Preparation instructions and recommendations.
			2. Storage and handling requirements and recommendations.
			3. Details of construction and fabrication.
			4. Installation methods.
		3. Shop Drawings: Include detailed plans, elevations, details of framing members, anchoring methods, required clearances, hardware, and accessories. Include relationship with adjacent construction.

\*\* NOTE TO SPECIFIER \*\* Delete selection samples if colors have already been selected.

* + 1. Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
		2. Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square, representing actual product, color, and patterns.
		3. Manufacturer's Certificates: Certify products meet or exceed specified requirements.
		4. Closeout Submittals: Provide manufacturer's maintenance instructions that include recommendations for periodic checking, adjustment and maintenance of all components.
	1. QUALITY ASSURANCE
		1. Manufacturer Qualifications: Company specializing in performing Work of this section with a minimum of five years experience in the fabrication and installation of security closures.
		2. Installer Qualifications: Installer Qualifications: Company specializing in performing Work of this section with minimum three years and approved by manufacturer.

\*\* NOTE TO SPECIFIER \*\* Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
			1. Finish areas designated by Architect.
			2. Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
			3. Refinish mock-up area as required to produce acceptable work.
	1. DELIVERY, STORAGE, AND HANDLING
		1. Store products in manufacturer's unopened packaging until ready for installation.
		2. Protect materials from exposure to moisture. Do not deliver until after wet work is complete and dry.
		3. Store materials in a dry, warm, ventilated weathertight location
	2. SEQUENCING
		1. Ensure that locating templates and other information required for installation of products of this section are furnished to affected trades in time to prevent interruption of construction progress.
		2. Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
	3. PROJECT CONDITIONS
		1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
	4. COORDINATION
		1. Coordinate Work with other operations and installation of adjacent materials to avoid damage to installed materials.
1. PRODUCTS
	1. MANUFACTURERS
		1. Acceptable Manufacturer: Wayne Dalton, which is located at: 2501 S. State Highway 121 Business, Suite 200; Lewisville, TX 75067; Toll Free Tel: (800) 827-3667; Email:[request info (info@wayne-dalton.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Wayne+Dalton&coid=36462&rep=&fax=&message=RE:%20Spec%20Question%20(08332way):%20%20&mf=); Web:<http://www.wayne-dalton.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
		2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Edit the following paragraphs as required and applicable to project requirements. Delete the paragraphs that are not applicable.

* 1. COILING WOOD COUNTER DOORS

\*\* NOTE TO SPECIFIER \*\* Wayne-Dalton Model 530 counter doors are available for openings with a maximum clear opening of 14 feet wide and 7 feet high. Wall thickness limitations are 3-5/8 inches minimum and 21 inches maximum.

* + 1. Coiling Wood Counter Doors: Wayne Dalton Model 530 Wood Rolling Counter Shutters.
		2. Curtain:
			1. Double rabbeted wood slats 1-3/4 inches high by 1/2 inch thick.
			2. Material:

\*\* NOTE TO SPECIFIER \*\* Select one of the following slat material paragraphs and delete the ones not required.

* + - * 1. Poplar.
				2. Red oak.
				3. Ash.
				4. As selected by the Architect from manufacturer's standard finishes.
		1. Guides:

\*\* NOTE TO SPECIFIER \*\* Select one of the following two paragraphs and delete the one not required.

* + - 1. Wood matching slat material.
			2. Aluminum guides with wool pile lining.
		1. Brackets: Metal plates with permanently sealed ball bearings designed to enclose ends of coil and provide support for counterbalance pipe at each end. Plated fabricated of:
			1. Steel 3/16 inch thick minimum.
		2. Counterbalance: Curtain is coiled on a pipe of sufficient size to carry door load with a deflection not to exceed 0.033 inch per foot of door span and to be correctly balanced by helical springs, oil tempered torsion type. Cast iron barrel plugs are used to anchor springs to tension shaft and pipe.
		3. Hood: Provide intermediate support brackets as required. Hood fabricated of:
			1. Wood matching slats.
		4. Finish: Clear finish as specified in Section 09900.

\*\* NOTE TO SPECIFIER \*\* Select one of the following paragraphs for manual operation or electric motor operation and delete the one not required.

* + 1. Manual Operation:

\*\* NOTE TO SPECIFIER \*\* Select one of the following manual operation paragraphs and delete the ones not required.

* + - 1. Manual push-up.
			2. Manual crank.

\*\* NOTE TO SPECIFIER \*\* Include the following paragraph if electric motor operation is required and delete if not required.

* + 1. Electric Motor Operation: Provide UL listed electric operator, size as recommended by manufacturer to move door in either direction at not less than 2/3 foot or more than 1 foot per second.
			1. Sensing Edge Protection:
				1. Electric sensing edge.
			2. Operator Controls:

\*\* NOTE TO SPECIFIER \*\* Select one of the following operation paragraphs and delete the one not required.

* + - * 1. Push-button operated control stations with open, close, and stop buttons.
				2. Key operation with open, close, and stop controls.
				3. Push-button and key operated control stations with open, close, and stop buttons.

\*\* NOTE TO SPECIFIER \*\* Select one of the following location paragraphs and delete the one not required.

* + - * 1. Controls for interior location.
				2. Controls for exterior location.
				3. Controls for both interior and exterior location.

\*\* NOTE TO SPECIFIER \*\* Select one of the following two paragraphs and delete the one not required.

* + - * 1. Controls surface mounted.
				2. Controls flush mounted.
		1. Locking
			1. Curtain to be locked at each end of bottom bar by concealed slide bolts which engage in a developed slot in each guide.

\*\* NOTE TO SPECIFIER \*\* Select the following option if required from the following paragraph. Delete if not applicable.

* + - 1. Provide cylinder lock at jambs or in center of bottom bar.

\*\* NOTE TO SPECIFIER \*\* Select the following option for power operated door from the following paragraph. Delete if not applicable.

* + - 1. Locks on electric-motor operated doors, shall be provided with electric interlocks to prevent operation when lock bolts are engaged in the guides.
		1. Mounting: Overhead Structure with:

\*\* NOTE TO SPECIFIER \*\* Select the one of the following options as required from the following paragraphs. Delete those not applicable.

* + - 1. Steel jambs.
			2. Wood jambs.
			3. Masonry jambs.
			4. Drywall over 16 gauge minimum steel studs or wood stud jambs.
1. EXECUTION
	1. EXAMINATION
		1. Verify opening sizes, tolerances and conditions are acceptable.
		2. Examine conditions of substrates, supports, and other conditions under which this work is to be performed.
		3. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
	2. PREPARATION
		1. Clean surfaces thoroughly prior to installation.
		2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
	3. INSTALLATION
		1. Install in accordance with manufacturer's instructions.
		2. Use anchorage devices to securely fasten assembly to wall construction and building framing without distortion or stress.
		3. Securely and rigidly brace components suspended from structure. Secure guides to structural members only.
		4. Fit and align assembly including hardware; level and plumb, to provide smooth operation.
		5. Coordinate installation of electrical service with Section 26 05 00 - Common Work Results for Electrical. Complete wiring from disconnect to unit components.
		6. Coordinate installation of sealants and backing materials at frame perimeter as specified in Section 07 90 00 - Joint Protection.
		7. Install perimeter trim and closures.
		8. Instruct Owner's personnel in proper operating procedures and maintenance schedule.
	4. ADJUSTING
		1. Test for proper operation and adjust as necessary to provide proper operation without binding or distortion.
		2. Adjust hardware and operating assemblies for smooth and noiseless operation.
	5. CLEANING
		1. Clean curtain and components using non-abrasive materials and methods recommended by manufacturer.
		2. Remove labels and visible markings.
	6. PROTECTION
		1. Protect installed products until completion of project.
		2. Touch-up, repair or replace damaged products before Substantial Completion.
	7. SCHEDULES

\*\* NOTE TO SPECIFIER \*\* Retain Paragraph below if required to suit project requirements. Identify products by name on the Drawings or use this paragraph to define the location of each type of material to be used. The following are some examples of schedule references. Edit as required to suit project or delete and identify products on the Drawings.

* + 1. :
		2. :

END OF SECTION